**TCP VS UDP**

**Part4:**

|  |  |  |
| --- | --- | --- |
| **Reasons** | **TCP or UDP** |  |
| TCP establishes a reliable connection using a three-way handshake (SYN, SYN-ACK, ACK) and ensures data delivery with acknowledgments and retransmissions. | **TCP** | Reliability and Connection Establishment |
| TCP guarantees data integrity and ordering through sequence numbers and acknowledgments, ensuring correct and complete data delivery. | **TCP** | Data Integrity and Ordering |

|  |  |  |
| --- | --- | --- |
| **UDP** | **TCP** |  |
| is suitable for applications where reliable data transmission is crucial and where data integrity and ordering must be guaranteed. These include web browsing, email, file transfers, and secure remote access | is suitable for applications where reliable data transmission is crucial and where data integrity and ordering must be guaranteed. These include web browsing, email, file transfers, and secure remote access | **Use Cases** |
| offers lower latency and faster data transfer due to its connectionless nature and minimal overhead, but it lacks guarantees for data delivery and ordering, which may lead to packet loss or duplication. | provides high reliability with guaranteed delivery and ordering of packets, but it comes with increased overhead and potential latency due to its connection-oriented nature. | **Performance** |